* If we look at a typical anodization curve, what is the approximate time constant?
  + Min/max?
* When the capacitor is anodizing, how does the Capacitance and series resistance change with time?
  + I am mostly interested with the endpoints to worry about a power spike at the beginning.
* Why do we want to anodize at a constant current?
  + From what I know a good bit of research has been done with anodizing at a constant voltage